## Using UA-101 Control Panel

### Menu

### "Driver" menu

Driver Settings...
  Opens the "UA-101 Driver Settings" dialog box. In the "UA-101 Driver Settings" dialog box you can adjust the buffer size and timing of the driver. For details on each item, refer to the "To change or verify settings."
Always on top
  Always displays UA-101 Control Panel in front of other windows.
About Driver & Control Panel...
  Displays the software version of the UA-101 driver and UA-101 Control Panel.
Exit
  Exits UA-101 Control Panel.

### "Device" menu

Set PATCH BAY...
  Opens a dialog box where you can make Patch Bay settings.
Load Memory of Device...
  Loads settings from the memory of the device.
Store Memory of Device...
  Stores settings into the memory of the device.
Reset Device...
  A dialog box will appear, allowing you to restore the device settings to the initial condition.
Select Device
  Selects the device for which you want to make settings.

### "Panel" menu

Cursor
  Left CH./Right CH.
    Moves the cursor location to left or right.
  INPUT 1, ... 10, OUTPUT 1, ... 10, MONITOR OUT 1,2
    Moves the cursor location to the specified channel.
MONITOR
  On/Off
    Switches MONITOR on/off at the cursor location.
  INPUT 1, ... 10, OUTPUT 1, ... 10
    Switches MONITOR on/off for the specified channel.
SOLO
  On/Off
    Switches SOLO on/off at the cursor location.
  INPUT 1, ... 10, OUTPUT 1, ... 10
    Switches SOLO on/off for the specified channel.
PAN
  Adjusts PAN at the cursor location.
VOLUME
  Adjusts VOLUME at the cursor location.
LINK
  On/Off
    Switches LINK on/off at the cursor location.
  INPUT 1-2, ... 9-10, OUTPUT 1-2, ... 9-10, MONITOR OUT 1-2
    Switches LINK on/off for the specified channel.
Reset setting
  Reset panel settings.

### Panel

### MONITOR

You can make the following adjustments for each channel of INPUT MONITOR 1, ... 10, OUTPUT MONITOR 1, ... 10, and MONITOR OUT (L/R).

SIGNAL
  Lights when signals are input or output via the various channels.
ON/OFF
  Switches MONITOR on/off.
SOLO
  Switches SOLO on/off.
PAN
  Drag the mouse to left/right to adjust PAN.
VOLUME
  Drag the mouse up/down to adjust VOLUME.
LINK
  Specify whether MONITOR on/off, SOLO, and VOLUME will be stereo-linked.
Cursor
  This is the yellow line upper the LINK button. Use the keyboard of your computer to edit the values at the cursor location. For the key assignments, refer to the "Panel" menu.

### Device Panel

This is displayed the bottom of the Panel window. It shows the state of the UA-101 front panel settings. From the left, this contains the following items.

Device select buttons
  These select the device.
SAMPLE RATE
  Indicates the sampling frequency of the current device.
CLOCK
  Indicates the type of synchronization clock for the current device.
DIRECT MONITOR
  MONO
    This will light if DIRECT MONITOR is set to monaural.
  SOFT CTRL
    This will light if DIRECT MONITOR settings can be adjusted from this control panel or ASIO-compatible application. If this is unlit, you can't perform DIRECT MONITOR operations.

### Dialog

### "PATCH BAY" dialog box

Specifies the output source for each OUTPUT.

Preset PATCH BAY
  Hard Thru
    "Hardware-thru's" the input from each INPUT to each OUTPUT.
  Initial setting
    Sends the output of each WAVE OUT to each OUTPUT.

### "Load Memory of Device" dialog box

Loads settings from the memory of the device.

### "Store Memory of Device" dialog box

Stores settings into the memory of the device.

### "Reset Device" dialog box

Select the items that you want to restore to their initial settings.

Copyright (C) 2009 Roland Corporation. All rights reserved.