1010 Driver Update for Windows 2000/XP

18-Oct-2004
Copyright 2004 ESI/Audiotrak, Ego Systems, Inc.    All Rights Reserved

======================================================================

             Thank you for choosing 1010 series. 

If you experience problems or need help with installing this update, 
consult the online Help or visit the ESI or Audiotrak Web site for
troubleshooting tips and answers to frequently asked questions, then
contact technical support on our web. 

                  WWW.ESI-PRO.COM    WWW.AUDIOTRAK.NET

======================================================================

This file may contains additions and changes to the printed manual. 
Please read this information before installing 1010 driver update.

======================================================================
INSTALLATION
======================================================================

Upgrading from a previous version 
======================================================================

Before removing the previous version, stop and close all applications 
that are using the 1010 driver.

A. Windows 2000/XP when the current driver is installed using auto 
   installation 

This installation process is based on the Windows XP system.
Installation on other systems is similar. However, if you experience
any difficulties please contact technical support.

   1. Click Start > Control Panel.
   2. In the Control Panel window, double-click Add or Remove
      Programs.
   3. Select 1010 Audio Driver VX.XX and remove the driver.
   4. Run Autoinst.exe from this driver package and follow on-screen
      instructions. Please ignore any Found New Hardware Wizard
      windows which may appear.

note: if the previous driver was not installed using auto install, it
has to be removed using infclear.exe before running autoinst.exe

B. Windows 2000/XP when the current driver was not installed using
   auto installation

   1. Run INFCLEAR.EXE.  
   2. Click Remove Driver.
   3. Click OK.
   4. On the System Properties Window, click Hardware > Device Manager
      > Sound, video and game controllers. Then, check the Device
      Manager to ensure 1010 drivers are removed.
   5. Click Restart and click OK to restart the computer.
   6. Ignore any Found New Hardware windows. Run autoinst.exe and 
      follow on-screen instructions.

C. Windows 2000/XP without auto installation
   1. Run INFCLEAR.EXE.  
   2. Click Remove Driver.
   3. Click OK.
   4. On the System Properties Window, click Hardware > Device Manager
      > Sound, video and game controllers. Then, check the Device
      Manager to ensure 1010 drivers are removed.
   5. Click Restart and click OK to restart the computer.
   6. After system restart, the Found New Hardware Wizard window will
      show up. Follow the installation instruction in the manual as if
      you are installing a new device. 

note: "The search for the best driver in these location" step should 
      point to the downloaded installation file directory.

If you experience problems restarting Windows after installing new
update, try to change the PCI slot of the ESP/MAYA1010.


                   < END OF FILE > 

