

README

YAMAHA DS2416,SW1000XG ASIO & MME Driver for Windows95/98/ME (File Set V4.0)
 (With support for GSIF Gigasampler format)

Thank you for choosing the DS2416/SW1000XG.

The YAMAHA DS2416/SW100XG Driver for Windows 95/98 is an ASIO/MME/GSIF audio 
driver with additional support for Nemesys/Endless Wave GSIF (Gigasampler 
Interface protocol) protocols to be used with a Yamaha DS2416/SW1000XG under 
Windows 95/98/ME. This driver is not designed for use under Windows 2000 or XP

The ASIO audio driver requires audio software, which supports ASIO. GSIF means
 software, which supports the Nemesys Gigasampler protocol.

============= Index ============================================ 
(1) License Agreement
(2) System environment
(3) Install and NOTES
(4) File set version history
(5) Yamaha Pro Audio products home page


(1) License Agreement
  PLEASE READ THIS DOCUMENT CAREFULLY BEFORE USING ANY SOFTWARE ON THIS
  MEDIA. THIS AGREEMENT LICENSES THE SOFTWARE TO YOU. BY USING THE SOFT-
  WARE, YOU ARE CONFIRMING YOUR ACCEPTANCE OF THE SOFTWARE AND AGREEING
  TO BECOME BOUND BY THE TERMS OF THIS AGREEMENT. IF YOU DO NOT WISH TO
  DO SO, PROMPTLY RETURN THE ENTIRE PACKAGE, INCLUDING THIS MEDIA, TO 
  THE PLACE WHERE YOU OBTAINED IT, FOR A FULL REFUND.

 1.Definitions.
  (a)"YAMAHA Software" means the software program and driver program in-
      cluded in the DS2416 package, and all related updates supplied by
      YAMAHA.
  (b) "YAMAHA Hardware" means the DS2416 digital mixing card and a con-
      nection cable.
  (c) "YAMAHA Product" means the YAMAHA Software, the YAMAHA Hardware,the
      related documentation, and all related updates supplied by YAMAHA.

 2.License.
  This agreement allows you, the purchaser, to use the YAMAHA Software 
  in conjunction with the YAMAHA Hardware.

 3. Restrictions.
  You may not decompile, reverse engineer, disassemble, or otherwaise 
  reduce the YAMAHA Software to a human-perceivable form, except to the
  limited extent expressly permitted by applicable law. You may not mod-
  ify, rent, resell for profit, distribute or create derivative works 
  based upon the YAMAHA Software or any part thereof. You may not export
  or reexport, directly or indirectly, the YAMAHA Product into any coun-
  try prohibited by the United States Export Administration Act and the 
  regulations thereunder.

 4.Ownership.
  The foregoing license gives you limited rights to use the YAMAHA Soft-
  ware. Although you own the media on which the YAMAHA Software is re-
  corded, you do not become the owner of, and YAMAHA retains title to,the
  YAMAHA Software and all copies thereof. All rights not specifically 
  granted in this agreement, including Federal and International Copy-
  rights, are reserved by YAMAHA.

 5. Disclaimer Of Warranty.
  The YAMAHA Software may contain errors that could cause failures or
  loss of data, and may be incomplete or contain inaccuracies. You ex-
  pressly acknowledge and agree that use of the YAMAHA Software is at
  your sole risk. The YAMAHA Software is provided "AS IS" and without
  warranty of any kind and YAMAHA EXPRESSLY DISCLAIM ALL WARRANTIES,EX-
  PRESS OR IMPLIED, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES
  OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE. YAMAHA DOES
  NOT WARRANT THAT THE FUNCTIONS CONTAINED IN THE YAMAHA SOFTWARE WILL
  MEET YOUR REQUIREMENTS, OR THAT THE OPERATION OF THE YAMAHA SOFTWARE
  WILL BE UNINTERRUPTED OR ERROR-FREE, OR THAT DEFECTS IN THE YAMAHA 
  SOFTWARE WILL BE CORRECTED. FURTHERMORE, YAMAHA DOES NOT WARRANT OR
  MAKE ANY REPRESENTATIONS REGARDING THE USE OR THE RESULTS OF THE USE
  OF THE YAMAHA SOFTWARE OR IN TERMS OF THEIR CORRECTNESS, ACCURACY,
  RELIABILITY, OR OTHERWISE.

 6. Term.
  This agreement is effective until terminated. You may terminate it at
  any time by destroying the YAMAHA Software together with all copies in
  any form. It will also terminate if you fail to comply with any term
  or condition in this agreemant.


----------------------------------------------------------------

(2)System environment

An IBM PC or compatible computers with a PCI bus compatible with 
the PCI 2.1/2.2 specifications. that runs Windows 9.x or ME Audio software
 supporting ASIO/MME.

(For GSIF support you will require Nemesys Gigasampler (see additional notes))
 Please note this driver is not intended to support GSIF under Windows 2000 or XP

----------------------------------------------------------------
(3)	Install

Follow these steps to update the driver.
I)	Displaying the file
1.	Select the Windows [View] menu, then [Folder Options].

The Option window opens.
2.	Select [View tab].
3.	Check the [View all files] checkbox.
4.	Press the [OK] button and close the Option window.


III)	Updating the driver
1.	Select [Start] menu, [Settings], then [Control Panel].

2.	Open [System] in the Control Panel.

3.	Select the [Device Manager] tab.

4.	Click the [+] mark next to [Sound, video, and game controllers].

5.	Select [Yamaha SW1000XG Sound System] and click the [Property] button.

6.	Select [Update Driver] to open [Update Driver Wizard].

7.	Select [No. Select driver from list.] for automatic detection,
        then click the [Next] button.

8.	Select YAMAHA SW1000XG Sound System as the model.

9.	Click the [Finish] button.

A dialog asking you to insert a disk appears. Insert the floppy disk that contains
 the new driver or point to the folder where the driver file is

10.Open the Setup file and follow the instructions on screen to install the new driver.

11.	Restart the computer.

12.  Open control panel and check with your device manager to see that the
  SW1000XG card and driver have been installed correctly.

13.  Now the driver has been updated.

 

To install ASIO Audio driver

If you are currently using ASIO driver version 2.0 or higher, new driver should be
 installed after deleting version 2.0 from [Add/Remove programs] in the Control Panel.

1.	Click the [Asio Setup.exe] and follow the guide.
2.	Launch the audio software which supports ASIO, 
3.	[ASIO SW+DS 32],[ASIO SW+DS 16] appears in the ASIO device menu. The Version number appears in the ASIO Control Panel

This driver allows to adjust Audio buffer size by clicking the "ASIO control Panel
 button" in [Audio system], when the  "ASIO SW+DS 32" is selected as audio I/O.


Notes:

Decreasing Audio buffer size will improve latency, however may cause noise problem
 depending on the PC environment.  In that case, increase audio buffer. 


Using the multiclient Gigasampler driver and the ASIO driver

The Gigasampler driver is automatically installed when you update your existing
 driver VXD and DLL files with this driver set. There is no special installation
 routine required for GSIF support other than this.


If you use the Gigasampler driver with the SW1000XG, you can use the ASIO driver with the DS2416 as well if you so wish (or vice-versa)

To achieve stable playback with the lowest latency value, we recommend the setting
 of 44.1kHz/stereo 16 or 32-bit.
(The format options vary depending on the application you are using with Gigasampler.)

Latency values for multichannel use of sub 30ms are now supported in this driver
 when used with GigaSampler. If you are currently using Gigasampler with the Direct X driver,
 please update to this driver and use the native GSIF support rather than Direct X support.



General notes

This driver is not designed for operation under Windows 2000 or XP

This driver supports GSIF 1.7 and GSIF 1.6 protocols, and will work with all versions
 of Gigasampler after version 1.6.

* You can use MME and GSIF exclusively for each channel if running multiple applications. 
In any Direct X application you should not try to assign channels which you are using for GSIF.

* You can use ASIO and GSIF exclusively for each board if you have 2 cards installed 
(DS & SW for example), and the cards are not connected (internally using the serial 
interface connecter).

* With the SW1000XG, You can use 16 or 32 bit data at 44.1kHz.

* With the DS2416, You can use 16 or 32 bit data at 44.1 and 48kHz. You have to set 
the same FS to GigaStudio/GigaSampler and YMIX (or your source sample clock reference
 setup in the applicable DS2416 application).  If you set a different FS between them,
 the output of DS2416 will be muted, and the card will not play.

(FS = Sample Frequency)


Limitations


* While you use Gigasampler, you will not be able to open control software for DS2416 
(Cubase, Logic or C-Console etc). You will have to open them before GigaStudio/GigaSampler
 is launched, then launch Gigasampler.

* If you have only one SW or DS board, you can use ASIO and GSIF at the same time using 
the virtual ports only, please bear this in mind.



The launch order for applications should be


For example

 Cubase
   1. Open Cubase. (or any main audio application)
   2. Open GigaStudio/GigaSampler.

 Logic
   1. Open DS2416 control soft (Patch/C_Console etc.)
   1. Open Logic. 
   2. Open GigaStudio/GigaSampler.


Please refer to your Gigasampler manual for setup with sequencers.

* GigaStudio on slower machines is a very high CPU/HDD load application, so SW1000XG
 may not receive all MIDI messages perfectly. By decreasing the number of Polyphonic 
notes (on slower machines (for example Pentium 166-200) on GigaStudio, you should be 
able to ease the problem.

Recommendation

* Yamaha do still recommend that in the case of using with a DS2416 you run Gigasampler
 as stand alone product on a separate PC. In the case of the SW1000XG this condition 
does not apply. This is due to the larger number of wave ports, and potential increased
 system load due to the greater number of ports.

----------------------------------------------------------------

(4) File set version history
      File Set V4.0 First released version.

----------------------------------------------------------------

(5)Yamaha Pro Audio products home page
  The following Web page provides you with information regarding the 
  DSP factory cards:
      URL= http://www.yamaha.co.jp/product/proaudio/

----------------------------------------------------------------

* Microsoft and Windows are registered trademarks of the Microsoft Cor-
  poration, USA, both in the USA and in other countries. 
* Company names and product names etc. in README.TXT are registered 
  trademarks or trademarks of their respective owners. 

(C) Copyright 1998-2001 YAMAHA CORPORATION
All Rights Reserved

===============================================================
End of file



